Engine
Clutch cover	M6x30	(11 off)	11Nm
Signal Generator Cover	M6x25	(5 off)		11Nm Sprocket Cover	M6x35	(3 off + 2 washers)		11Nm Starter Clutch Cover	M6x30	(9 off)		11Nm Cam Cover Bolts	M8 and M7	(2 off and 8 off)	20Nm and 14Nm

Handlebars
Clutch Master Cylinder Bracket	M6x20	(2 off)	10Nm
Clutch Master Cylinder Cap	M4x12 c/sunk        (2 off)		- Clutch Cutout Switch @ lever	M4x12 button         (1 off + spring and flat washer)		- Front Brake Master Cylinder Bracket M6x25	(2 off)	10Nm
Front Brake Master Cylinder Cap        M4x12 c/sunk       (2 off)		- Front Brake Switch @ lever	M4x12 button         (1 off + spring and flat washer)		- Handlebar clamps	M8X30	(4 off + spring washers)	23Nm
Switchgear	M5x25 button	(1 off)	-
Switchgear	M5x45 button	(3 off)	-
Throttle Housing	M5X25	(2 off)	-

Front Forks and Front Brakes
Bottom Yoke Pinch Bolts	M8x35	(4 off + spring washers)	23Nm Front Brake Splitter	M6x12	(1 off + flat washer)	23Nm Front Brake Splitter	M6x20	(1 off + flat washer)	23Nm Fork Leg Pinch Bolts (front axle)        M8x45	(4 off)	23Nm
Front Brake Caliper Housing	M8x40	(8 off)	21Nm
Front Brake Caliper Mount	M8x30	(4 off)	26Nm
Front Brake Bleed Nipples	M7x1.00 pitch	(2 off)	8Nm
Front Mudguard	M5X35	(4 off)		- Top Yoke Pinch Bolts	M8x35	(2 off + spring washers)	23Nm

Frame
Oil Cooler Mounting Bracket	M6x35	(2 off + flat washers)	10Nm Side Stand Switch	M6x20	(2 off)		-
Top Rear Engine Mount Bolt	M10x155	(1 off)	85Nm
Bottom Rear Engine Mount Bolt	M12x140	(1 off)	88Nm Removable frame section bolts	M10x25	(6 off, 1.25 pitch)	50Nm

Swingarm, Rear Brake
Chain Adjustment Bolt	M8x50	(2 off)	-
Chainguard (rear bolt)	M6x10 button	(1 off)	-
Chainguard (front bolt)	M6x25 button	(1 off)		- Rear Axle Nut	M25x1.5	(36mm socket size)	100Nm Rear Sprocket Nuts	M12x1.25 pitch       (5 off)	102Nm
Rear Brake Caliper Housing	M10x45 1.25 pitch  (2 off)	37Nm
Rear Brake Caliper Mount	M8X30	(2 off)	26Nm
Rear Brake Nipples	M8x1.25 pitch	(2 off)	8Nm
Lower Rear Suspension Mount bolt  M10x45	(2 off)	
  Lower Rear Suspension Mount nut   M10		  (2 off)				    34Nm

Exhaust
[bookmark: _GoBack]Exhaust clamps	M8x25	(8 off)	23Nm Exhaust pipes to link pipes	M8x35	(2 off + washers)	20Nm Exhaust silencer can (to frame)        M8X40	(2 off + washers + flange nuts) 	23Nm

Cosmetic
Grab Rail Bolts	M8x70 (2 off) AND M6x45 (2 off)
